Slaking Build Notes
Build the forehead first, moving down the face. Be sure to have the mouth ridge (2) 
cut out before working on the main piece of the face (3) so that 
they can be connected as soon as possible. After the face is built, attach the teeth and nose
and work toward the back of the head. 9 and 10 go directly on top of the head after it is built.

Now work down the body, building the arms from the cuff in, and connecting when complete.
The hands can be inserted at any time after the arms are built,
since they just get pushed into the hole with a little glue
for support. Move down towards the bottom, building the legs from the body down, and 
inserting the feet in a way similar to the hands. 

Be sure to trim all the cuffs (both arms and legs) so that there is no more white. 
Do the same with the neck cuff, although be more careful; as the cuff is actually
just a shade of white. Attach the cuff (38) at any time after the arms are built; 
it doesn't matter when so long as it isn't obstructing anything you're 
currently building.  
