Glue the separate "shell" pieces, attaching the spikes as soon as possible. All pieces should be ready but one - piece 18, the one with the tabless shell segment. Glue the pieces to the tabbed eye, then close by gluing the tabless segment of piece 18. The shell should be done. Finish by attaching the tabless eye to the shell.